From 7046dc2a485b2b2ec993d7c933820c8ae2b45718 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Wed, 20 Jan 2016 10:14:39 +0100
Subject: [PATCH 35/91] soc: mediatek: PMIC wrap: WRAP_INT_EN needs a
 different bitmask for MT2701/7623

MT2701 and MT7623 use a different bitmask for PWRAP_INT_EN.

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 drivers/soc/mediatek/mtk-pmic-wrap.c |    5 ++++-
 1 file changed, 4 insertions(+), 1 deletion(-)

diff --git a/drivers/soc/mediatek/mtk-pmic-wrap.c b/drivers/soc/mediatek/mtk-pmic-wrap.c
index 22c89e9..9df1135 100644
--- a/drivers/soc/mediatek/mtk-pmic-wrap.c
+++ b/drivers/soc/mediatek/mtk-pmic-wrap.c
@@ -371,6 +371,7 @@ struct pmic_wrapper_type {
 	int *regs;
 	enum pwrap_type type;
 	u32 arb_en_all;
+	u32 int_en_all;
 	int (*init_reg_clock)(struct pmic_wrapper *wrp);
 	int (*init_soc_specific)(struct pmic_wrapper *wrp);
 };
@@ -825,6 +826,7 @@ static struct pmic_wrapper_type pwrap_mt8135 = {
 	.regs = mt8135_regs,
 	.type = PWRAP_MT8135,
 	.arb_en_all = 0x1ff,
+	.int_en_all = ~(BIT(31) | BIT(1)),
 	.init_reg_clock = pwrap_mt8135_init_reg_clock,
 	.init_soc_specific = pwrap_mt8135_init_soc_specific,
 };
@@ -833,6 +835,7 @@ static struct pmic_wrapper_type pwrap_mt8173 = {
 	.regs = mt8173_regs,
 	.type = PWRAP_MT8173,
 	.arb_en_all = 0x3f,
+	.int_en_all = ~(BIT(31) | BIT(1)),
 	.init_reg_clock = pwrap_mt8173_init_reg_clock,
 	.init_soc_specific = pwrap_mt8173_init_soc_specific,
 };
@@ -946,7 +949,7 @@ static int pwrap_probe(struct platform_device *pdev)
 			PWRAP_WDT_SRC_MASK_NO_STAUPD : PWRAP_WDT_SRC_MASK_ALL;
 	pwrap_writel(wrp, wdt_src, PWRAP_WDT_SRC_EN);
 	pwrap_writel(wrp, 0x1, PWRAP_TIMER_EN);
-	pwrap_writel(wrp, ~((1 << 31) | (1 << 1)), PWRAP_INT_EN);
+	pwrap_writel(wrp, wrp->master->int_en_all, PWRAP_INT_EN);
 
 	irq = platform_get_irq(pdev, 0);
 	ret = devm_request_irq(wrp->dev, irq, pwrap_interrupt, IRQF_TRIGGER_HIGH,
-- 
1.7.10.4

