#!/bin/sh
#
# Copyright (C) 2015 OpenWrt.org
#

. /lib/functions/uci-defaults.sh
. /lib/ipq806x.sh

board_config_update

board=$(ipq806x_board_name)

case "$board" in
d7800 |\
r7500)
	ucidef_set_led_usbdev "usb1" "USB 1" "r7500:white:usb1" "1-1"
	ucidef_set_led_usbdev "usb2" "USB 2" "r7500:white:usb3" "3-1"
	ucidef_set_led_netdev "wan" "WAN" "r7500:white:wan" "eth0"
	ucidef_set_led_ide "esata" "eSATA" "r7500:amber:esata"
	ucidef_set_led_default "wps" "WPS" "r7500:white:wps" "0"
	ucidef_set_led_default "rfkill" "rfkill" "r7500:white:rfkill" "0"
	;;
*)
	;;
esac

board_config_flush

exit 0
