From 39929365081d5aa7c311ee8325c7f1a0ffb88a76 Mon Sep 17 00:00:00 2001
From: Kurt Mahan <kmahan@freescale.com>
Date: Mon, 7 Jul 2008 23:37:30 -0600
Subject: [PATCH] Enable uboot bootargs.

LTIBName: mcfv4e-uboot-bootargs
Signed-off-by: Kurt Mahan <kmahan@freescale.com>
---
 arch/m68k/coldfire/config.c |    5 -----
 1 files changed, 0 insertions(+), 5 deletions(-)

--- a/arch/m68k/coldfire/config.c
+++ b/arch/m68k/coldfire/config.c
@@ -196,7 +196,6 @@ asmlinkage void __init cf_early_init(voi
 	m68k_memory[m68k_num_memory].addr = CONFIG_SDRAM_BASE;
 	m68k_memory[m68k_num_memory++].size = CONFIG_SDRAM_SIZE;
 
-#if 0
 	if (!uboot_commandline(m68k_command_line)) {
 #if defined(CONFIG_BOOTPARAM)
 		strncpy(m68k_command_line, CONFIG_BOOTPARAM_STRING, CL_SIZE-1);
@@ -204,10 +203,6 @@ asmlinkage void __init cf_early_init(voi
 		strcpy(m68k_command_line, DEFAULT_COMMAND_LINE);
 #endif
 	}
-#endif
-/* JKM -- temporary! */
-strcpy(m68k_command_line, DEFAULT_COMMAND_LINE);
-/* JKM -- temporary! */
 
 #if defined(CONFIG_BLK_DEV_INITRD)
 	/* add initrd image */
