--- a/arch/arm/mach-mx2/Kconfig
+++ b/arch/arm/mach-mx2/Kconfig
@@ -27,6 +27,12 @@ config MACH_MX21ADS
 	  Include support for MX21ADS platform. This includes specific
 	  configurations for the board and its peripherals.
 
+config MACH_VP6500
+	bool "Phillips VP6500 VoIP phone"
+	depends on MACH_MX21
+	help
+	  Include support for the Phillips VP6500 VoIP phone.
+
 config MACH_MX27ADS
 	bool "MX27ADS platform"
 	depends on MACH_MX27
--- a/arch/arm/mach-mx2/Makefile
+++ b/arch/arm/mach-mx2/Makefile
@@ -21,3 +21,4 @@ obj-$(CONFIG_MACH_CPUIMX27) += mach-cpui
 obj-$(CONFIG_MACH_EUKREA_MBIMX27_BASEBOARD) += eukrea_mbimx27-baseboard.o
 obj-$(CONFIG_MACH_PCA100) += mach-pca100.o
 obj-$(CONFIG_MACH_MXT_TD60) += mach-mxt_td60.o
+obj-$(CONFIG_MACH_VP6500) += mach-vp6500.o
