From 699c57a18b40ffbe1763915acdc1a3e4fb539d01 Mon Sep 17 00:00:00 2001
From: Hauke Mehrtens <hauke@hauke-m.de>
Date: Fri, 13 Jan 2012 17:42:15 +0100
Subject: [PATCH 29/32] bcma: add new PCI ID

This ID was found on the PCIe wireless card on the board of a Netgear
WNDR3400 using a bcm4716. The device with this ID is identified by b43
as "Broadcom 43224 WLAN".

Signed-off-by: Hauke Mehrtens <hauke@hauke-m.de>
---
 drivers/bcma/host_pci.c |    1 +
 1 files changed, 1 insertions(+), 0 deletions(-)

--- a/drivers/bcma/host_pci.c
+++ b/drivers/bcma/host_pci.c
@@ -269,6 +269,7 @@ static DEFINE_PCI_DEVICE_TABLE(bcma_pci_
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4353) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4357) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4727) },
+	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0xa8d8) },
 	{ 0, },
 };
 MODULE_DEVICE_TABLE(pci, bcma_pci_bridge_tbl);
