From e5ae2eed68a7ccd406bde12ecfc12c88a52aeb06 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Thu, 8 Mar 2012 13:13:31 +0100
Subject: [PATCH 49/70] MIPS: lantiq: pci: give xway pci support its own
 kbuild symbol

---
 arch/mips/lantiq/Kconfig |    5 +++++
 arch/mips/pci/Makefile   |    2 +-
 2 files changed, 6 insertions(+), 1 deletions(-)

--- a/arch/mips/lantiq/Kconfig
+++ b/arch/mips/lantiq/Kconfig
@@ -19,8 +19,13 @@ config SOC_XWAY
 
 config SOC_FALCON
 	bool "FALCON"
+
 endchoice
 
+config PCI_LANTIQ
+	bool "PCI Support"
+	depends on SOC_XWAY && PCI
+
 source "arch/mips/lantiq/xway/Kconfig"
 source "arch/mips/lantiq/falcon/Kconfig"
 
--- a/arch/mips/pci/Makefile
+++ b/arch/mips/pci/Makefile
@@ -41,7 +41,7 @@ obj-$(CONFIG_SIBYTE_SB1250)	+= fixup-sb1
 obj-$(CONFIG_SIBYTE_BCM112X)	+= fixup-sb1250.o pci-sb1250.o
 obj-$(CONFIG_SIBYTE_BCM1x80)	+= pci-bcm1480.o pci-bcm1480ht.o
 obj-$(CONFIG_SNI_RM)		+= fixup-sni.o ops-sni.o
-obj-$(CONFIG_SOC_XWAY)		+= pci-lantiq.o ops-lantiq.o
+obj-$(CONFIG_PCI_LANTIQ)	+= pci-lantiq.o ops-lantiq.o
 obj-$(CONFIG_TANBAC_TB0219)	+= fixup-tb0219.o
 obj-$(CONFIG_TANBAC_TB0226)	+= fixup-tb0226.o
 obj-$(CONFIG_TANBAC_TB0287)	+= fixup-tb0287.o
