From 875a7139535da541aa2e9de308b3f6f791a131d0 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Tue, 20 Mar 2012 09:44:27 +0100
Subject: [PATCH 63/70] MIPS: lantiq: irqs were not cleared properly on boot

---
 arch/mips/lantiq/irq.c |   10 +++++-----
 1 files changed, 5 insertions(+), 5 deletions(-)

--- a/arch/mips/lantiq/irq.c
+++ b/arch/mips/lantiq/irq.c
@@ -326,12 +326,12 @@ void __init arch_init_irq(void)
 			panic("Failed to remap eiu memory\n");
 	}
 
-	/* make sure all irqs are turned off by default */
-	for (i = 0; i < 5; i++)
+	for (i = 0; i < 5; i++) {
+		/* make sure all irqs are turned off by default */
 		ltq_icu_w32(0, LTQ_ICU_IM0_IER + (i * LTQ_ICU_OFFSET));
-
-	/* clear all possibly pending interrupts */
-	ltq_icu_w32(~0, LTQ_ICU_IM0_ISR + (i * LTQ_ICU_OFFSET));
+		/* clear all possibly pending interrupts */
+		ltq_icu_w32(~0, LTQ_ICU_IM0_ISR + (i * LTQ_ICU_OFFSET));
+	}
 
 	mips_cpu_irq_init();
 
