From 57f251cd4c0172cd080ca83994e794b1b6515148 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Noralf=20Tr=C3=B8nnes?= <noralf@tronnes.org>
Date: Sat, 3 Jul 2021 16:13:20 +0200
Subject: [PATCH] drm/gud: Add Raspberry Pi Pico ID
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

[ drm-misc commit b3f4ef669357d5b9a2c5e8c33e3967a2070db7f9 ]

Add VID/PID for the Raspberry Pi Pico implementation.
Source: https://github.com/notro/gud-pico

Cc: Linus Walleij <linus.walleij@linaro.org>
Signed-off-by: Noralf Trønnes <noralf@tronnes.org>
Reviewed-by: Peter Stuge <peter@stuge.se>
Link: https://patchwork.freedesktop.org/patch/msgid/20210703141321.35494-1-noralf@tronnes.org
---
 drivers/gpu/drm/gud/gud_drv.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/gpu/drm/gud/gud_drv.c
+++ b/drivers/gpu/drm/gud/gud_drv.c
@@ -674,6 +674,7 @@ static int gud_resume(struct usb_interfa
 
 static const struct usb_device_id gud_id_table[] = {
 	{ USB_DEVICE_INTERFACE_CLASS(0x1d50, 0x614d, USB_CLASS_VENDOR_SPEC) },
+	{ USB_DEVICE_INTERFACE_CLASS(0x16d0, 0x10a9, USB_CLASS_VENDOR_SPEC) },
 	{ }
 };
 
