From 729fd05aac22cdf1e502fbf1bf80e5ebba0d9fbc Mon Sep 17 00:00:00 2001
From: Russell King <rmk+kernel@armlinux.org.uk>
Date: Tue, 3 Dec 2019 17:48:28 +0000
Subject: [PATCH] net: sfp: fix unbind

When unbinding, we don't correctly tear down the module state, leaving
(for example) the hwmon registration behind. Ensure everything is
properly removed by sending a remove event at unbind.

Fixes: 6b0da5c9c1a3 ("net: sfp: track upstream's attachment state in state machine")
Signed-off-by: Russell King <rmk+kernel@armlinux.org.uk>
---
 drivers/net/phy/sfp.c | 4 ++++
 1 file changed, 4 insertions(+)

--- a/drivers/net/phy/sfp.c
+++ b/drivers/net/phy/sfp.c
@@ -2431,6 +2431,10 @@ static int sfp_remove(struct platform_de
 
 	sfp_unregister_socket(sfp->sfp_bus);
 
+	rtnl_lock();
+	sfp_sm_event(sfp, SFP_E_REMOVE);
+	rtnl_unlock();
+
 	return 0;
 }
 
