From f9681320a1c1caed9c899acfefcb308ac7c911d1 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime.ripard@free-electrons.com>
Date: Fri, 1 May 2015 22:39:45 +0200
Subject: [PATCH] Add cubieboard2 audio codec

Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 arch/arm/boot/dts/sun7i-a20-cubieboard2.dts | 7 +++++++
 1 file changed, 7 insertions(+)

--- a/arch/arm/boot/dts/sun7i-a20-cubieboard2.dts
+++ b/arch/arm/boot/dts/sun7i-a20-cubieboard2.dts
@@ -180,6 +180,13 @@
 
 #include "axp209.dtsi"
 
+&codec {
+	routing =
+		"Headphone Jack", "HP Left",
+		"Headphone Jack", "HP Right";
+	status = "okay";
+};
+
 &cpu0 {
 	cpu-supply = <&reg_dcdc2>;
 };
