From 52dde352cc7a558eab85458c3f7ab90dc652f761 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Fri, 8 Jan 2016 04:09:43 +0100
Subject: [PATCH 45/91] mfd: mt6397: add MT6323 support to MT6397 driver

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 drivers/mfd/mt6397-core.c            |   20 ++
 include/linux/mfd/mt6323/core.h      |   36 +++
 include/linux/mfd/mt6323/registers.h |  408 ++++++++++++++++++++++++++++++++++
 3 files changed, 464 insertions(+)
 create mode 100644 include/linux/mfd/mt6323/core.h
 create mode 100644 include/linux/mfd/mt6323/registers.h

diff --git a/drivers/mfd/mt6397-core.c b/drivers/mfd/mt6397-core.c
index aa91606..8234cd3 100644
--- a/drivers/mfd/mt6397-core.c
+++ b/drivers/mfd/mt6397-core.c
@@ -19,11 +19,14 @@
 #include <linux/regmap.h>
 #include <linux/mfd/core.h>
 #include <linux/mfd/mt6397/core.h>
+#include <linux/mfd/mt6323/core.h>
 #include <linux/mfd/mt6397/registers.h>
+#include <linux/mfd/mt6323/registers.h>
 
 #define MT6397_RTC_BASE		0xe000
 #define MT6397_RTC_SIZE		0x3e
 
+#define MT6323_CID_CODE		0x23
 #define MT6391_CID_CODE		0x91
 #define MT6397_CID_CODE		0x97
 
@@ -40,6 +43,13 @@ static const struct resource mt6397_rtc_resources[] = {
 	},
 };
 
+static const struct mfd_cell mt6323_devs[] = {
+	{
+		.name = "mt6323-regulator",
+		.of_compatible = "mediatek,mt6323-regulator"
+	},
+};
+
 static const struct mfd_cell mt6397_devs[] = {
 	{
 		.name = "mt6397-rtc",
@@ -261,6 +271,15 @@ static int mt6397_probe(struct platform_device *pdev)
 	}
 
 	switch (id & 0xff) {
+	case MT6323_CID_CODE:
+		pmic->int_con[0] = MT6323_INT_CON0;
+		pmic->int_con[1] = MT6323_INT_CON1;
+		pmic->int_status[0] = MT6323_INT_STATUS0;
+		pmic->int_status[1] = MT6323_INT_STATUS1;
+		ret = mfd_add_devices(&pdev->dev, -1, mt6323_devs,
+				ARRAY_SIZE(mt6323_devs), NULL, 0, NULL);
+		break;
+
 	case MT6397_CID_CODE:
 	case MT6391_CID_CODE:
 		pmic->int_con[0] = MT6397_INT_CON0;
@@ -302,6 +321,7 @@ static int mt6397_remove(struct platform_device *pdev)
 
 static const struct of_device_id mt6397_of_match[] = {
 	{ .compatible = "mediatek,mt6397" },
+	{ .compatible = "mediatek,mt6323" },
 	{ }
 };
 MODULE_DEVICE_TABLE(of, mt6397_of_match);
diff --git a/include/linux/mfd/mt6323/core.h b/include/linux/mfd/mt6323/core.h
new file mode 100644
index 0000000..06d0ec3
--- /dev/null
+++ b/include/linux/mfd/mt6323/core.h
@@ -0,0 +1,36 @@
+/*
+ * Copyright (c) 2016 Chen Zhong <chen.zhong@mediatek.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#ifndef __MFD_MT6323_CORE_H__
+#define __MFD_MT6323_CORE_H__
+
+enum MT6323_IRQ_STATUS_numbers {
+	MT6323_IRQ_STATUS_SPKL_AB = 0,
+	MT6323_IRQ_STATUS_SPKL,
+	MT6323_IRQ_STATUS_BAT_L,
+	MT6323_IRQ_STATUS_BAT_H,
+	MT6323_IRQ_STATUS_WATCHDOG,
+	MT6323_IRQ_STATUS_PWRKEY,
+	MT6323_IRQ_STATUS_THR_L,
+	MT6323_IRQ_STATUS_THR_H,
+	MT6323_IRQ_STATUS_VBATON_UNDET,
+	MT6323_IRQ_STATUS_BVALID_DET,
+	MT6323_IRQ_STATUS_CHRDET,
+	MT6323_IRQ_STATUS_OV,
+	MT6323_IRQ_STATUS_LDO = 16,
+	MT6323_IRQ_STATUS_FCHRKEY,
+	MT6323_IRQ_STATUS_ACCDET,
+	MT6323_IRQ_STATUS_AUDIO,
+	MT6323_IRQ_STATUS_RTC,
+	MT6323_IRQ_STATUS_VPROC,
+	MT6323_IRQ_STATUS_VSYS,
+	MT6323_IRQ_STATUS_VPA,
+	MT6323_IRQ_STATUS_NR,
+};
+
+#endif /* __MFD_MT6323_CORE_H__ */
diff --git a/include/linux/mfd/mt6323/registers.h b/include/linux/mfd/mt6323/registers.h
new file mode 100644
index 0000000..160f3c0
--- /dev/null
+++ b/include/linux/mfd/mt6323/registers.h
@@ -0,0 +1,408 @@
+/*
+ * Copyright (c) 2016 Chen Zhong <chen.zhong@mediatek.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#ifndef __MFD_MT6323_REGISTERS_H__
+#define __MFD_MT6323_REGISTERS_H__
+
+/* PMIC Registers */
+#define MT6323_CHR_CON0           0x0000
+#define MT6323_CHR_CON1           0x0002
+#define MT6323_CHR_CON2           0x0004
+#define MT6323_CHR_CON3           0x0006
+#define MT6323_CHR_CON4           0x0008
+#define MT6323_CHR_CON5           0x000A
+#define MT6323_CHR_CON6           0x000C
+#define MT6323_CHR_CON7           0x000E
+#define MT6323_CHR_CON8           0x0010
+#define MT6323_CHR_CON9           0x0012
+#define MT6323_CHR_CON10          0x0014
+#define MT6323_CHR_CON11          0x0016
+#define MT6323_CHR_CON12          0x0018
+#define MT6323_CHR_CON13          0x001A
+#define MT6323_CHR_CON14          0x001C
+#define MT6323_CHR_CON15          0x001E
+#define MT6323_CHR_CON16          0x0020
+#define MT6323_CHR_CON17          0x0022
+#define MT6323_CHR_CON18          0x0024
+#define MT6323_CHR_CON19          0x0026
+#define MT6323_CHR_CON20          0x0028
+#define MT6323_CHR_CON21          0x002A
+#define MT6323_CHR_CON22          0x002C
+#define MT6323_CHR_CON23          0x002E
+#define MT6323_CHR_CON24          0x0030
+#define MT6323_CHR_CON25          0x0032
+#define MT6323_CHR_CON26          0x0034
+#define MT6323_CHR_CON27          0x0036
+#define MT6323_CHR_CON28          0x0038
+#define MT6323_CHR_CON29          0x003A
+#define MT6323_STRUP_CON0         0x003C
+#define MT6323_STRUP_CON2         0x003E
+#define MT6323_STRUP_CON3         0x0040
+#define MT6323_STRUP_CON4         0x0042
+#define MT6323_STRUP_CON5         0x0044
+#define MT6323_STRUP_CON6         0x0046
+#define MT6323_STRUP_CON7         0x0048
+#define MT6323_STRUP_CON8         0x004A
+#define MT6323_STRUP_CON9         0x004C
+#define MT6323_STRUP_CON10        0x004E
+#define MT6323_STRUP_CON11        0x0050
+#define MT6323_SPK_CON0           0x0052
+#define MT6323_SPK_CON1           0x0054
+#define MT6323_SPK_CON2           0x0056
+#define MT6323_SPK_CON6           0x005E
+#define MT6323_SPK_CON7           0x0060
+#define MT6323_SPK_CON8           0x0062
+#define MT6323_SPK_CON9           0x0064
+#define MT6323_SPK_CON10          0x0066
+#define MT6323_SPK_CON11          0x0068
+#define MT6323_SPK_CON12          0x006A
+#define MT6323_CID                0x0100
+#define MT6323_TOP_CKPDN0         0x0102
+#define MT6323_TOP_CKPDN0_SET     0x0104
+#define MT6323_TOP_CKPDN0_CLR     0x0106
+#define MT6323_TOP_CKPDN1         0x0108
+#define MT6323_TOP_CKPDN1_SET     0x010A
+#define MT6323_TOP_CKPDN1_CLR     0x010C
+#define MT6323_TOP_CKPDN2         0x010E
+#define MT6323_TOP_CKPDN2_SET     0x0110
+#define MT6323_TOP_CKPDN2_CLR     0x0112
+#define MT6323_TOP_RST_CON        0x0114
+#define MT6323_TOP_RST_CON_SET    0x0116
+#define MT6323_TOP_RST_CON_CLR    0x0118
+#define MT6323_TOP_RST_MISC       0x011A
+#define MT6323_TOP_RST_MISC_SET   0x011C
+#define MT6323_TOP_RST_MISC_CLR   0x011E
+#define MT6323_TOP_CKCON0         0x0120
+#define MT6323_TOP_CKCON0_SET     0x0122
+#define MT6323_TOP_CKCON0_CLR     0x0124
+#define MT6323_TOP_CKCON1         0x0126
+#define MT6323_TOP_CKCON1_SET     0x0128
+#define MT6323_TOP_CKCON1_CLR     0x012A
+#define MT6323_TOP_CKTST0         0x012C
+#define MT6323_TOP_CKTST1         0x012E
+#define MT6323_TOP_CKTST2         0x0130
+#define MT6323_TEST_OUT           0x0132
+#define MT6323_TEST_CON0          0x0134
+#define MT6323_TEST_CON1          0x0136
+#define MT6323_EN_STATUS0         0x0138
+#define MT6323_EN_STATUS1         0x013A
+#define MT6323_OCSTATUS0          0x013C
+#define MT6323_OCSTATUS1          0x013E
+#define MT6323_PGSTATUS           0x0140
+#define MT6323_CHRSTATUS          0x0142
+#define MT6323_TDSEL_CON          0x0144
+#define MT6323_RDSEL_CON          0x0146
+#define MT6323_SMT_CON0           0x0148
+#define MT6323_SMT_CON1           0x014A
+#define MT6323_SMT_CON2           0x014C
+#define MT6323_SMT_CON3           0x014E
+#define MT6323_SMT_CON4           0x0150
+#define MT6323_DRV_CON0           0x0152
+#define MT6323_DRV_CON1           0x0154
+#define MT6323_DRV_CON2           0x0156
+#define MT6323_DRV_CON3           0x0158
+#define MT6323_DRV_CON4           0x015A
+#define MT6323_SIMLS1_CON         0x015C
+#define MT6323_SIMLS2_CON         0x015E
+#define MT6323_INT_CON0           0x0160
+#define MT6323_INT_CON0_SET       0x0162
+#define MT6323_INT_CON0_CLR       0x0164
+#define MT6323_INT_CON1           0x0166
+#define MT6323_INT_CON1_SET       0x0168
+#define MT6323_INT_CON1_CLR       0x016A
+#define MT6323_INT_MISC_CON       0x016C
+#define MT6323_INT_MISC_CON_SET   0x016E
+#define MT6323_INT_MISC_CON_CLR   0x0170
+#define MT6323_INT_STATUS0        0x0172
+#define MT6323_INT_STATUS1        0x0174
+#define MT6323_OC_GEAR_0          0x0176
+#define MT6323_OC_GEAR_1          0x0178
+#define MT6323_OC_GEAR_2          0x017A
+#define MT6323_OC_CTL_VPROC       0x017C
+#define MT6323_OC_CTL_VSYS        0x017E
+#define MT6323_OC_CTL_VPA         0x0180
+#define MT6323_FQMTR_CON0         0x0182
+#define MT6323_FQMTR_CON1         0x0184
+#define MT6323_FQMTR_CON2         0x0186
+#define MT6323_RG_SPI_CON         0x0188
+#define MT6323_DEW_DIO_EN         0x018A
+#define MT6323_DEW_READ_TEST      0x018C
+#define MT6323_DEW_WRITE_TEST     0x018E
+#define MT6323_DEW_CRC_SWRST      0x0190
+#define MT6323_DEW_CRC_EN         0x0192
+#define MT6323_DEW_CRC_VAL        0x0194
+#define MT6323_DEW_DBG_MON_SEL    0x0196
+#define MT6323_DEW_CIPHER_KEY_SEL 0x0198
+#define MT6323_DEW_CIPHER_IV_SEL  0x019A
+#define MT6323_DEW_CIPHER_EN      0x019C
+#define MT6323_DEW_CIPHER_RDY     0x019E
+#define MT6323_DEW_CIPHER_MODE    0x01A0
+#define MT6323_DEW_CIPHER_SWRST   0x01A2
+#define MT6323_DEW_RDDMY_NO       0x01A4
+#define MT6323_DEW_RDATA_DLY_SEL  0x01A6
+#define MT6323_BUCK_CON0          0x0200
+#define MT6323_BUCK_CON1          0x0202
+#define MT6323_BUCK_CON2          0x0204
+#define MT6323_BUCK_CON3          0x0206
+#define MT6323_BUCK_CON4          0x0208
+#define MT6323_BUCK_CON5          0x020A
+#define MT6323_VPROC_CON0         0x020C
+#define MT6323_VPROC_CON1         0x020E
+#define MT6323_VPROC_CON2         0x0210
+#define MT6323_VPROC_CON3         0x0212
+#define MT6323_VPROC_CON4         0x0214
+#define MT6323_VPROC_CON5         0x0216
+#define MT6323_VPROC_CON7         0x021A
+#define MT6323_VPROC_CON8         0x021C
+#define MT6323_VPROC_CON9         0x021E
+#define MT6323_VPROC_CON10        0x0220
+#define MT6323_VPROC_CON11        0x0222
+#define MT6323_VPROC_CON12        0x0224
+#define MT6323_VPROC_CON13        0x0226
+#define MT6323_VPROC_CON14        0x0228
+#define MT6323_VPROC_CON15        0x022A
+#define MT6323_VPROC_CON18        0x0230
+#define MT6323_VSYS_CON0          0x0232
+#define MT6323_VSYS_CON1          0x0234
+#define MT6323_VSYS_CON2          0x0236
+#define MT6323_VSYS_CON3          0x0238
+#define MT6323_VSYS_CON4          0x023A
+#define MT6323_VSYS_CON5          0x023C
+#define MT6323_VSYS_CON7          0x0240
+#define MT6323_VSYS_CON8          0x0242
+#define MT6323_VSYS_CON9          0x0244
+#define MT6323_VSYS_CON10         0x0246
+#define MT6323_VSYS_CON11         0x0248
+#define MT6323_VSYS_CON12         0x024A
+#define MT6323_VSYS_CON13         0x024C
+#define MT6323_VSYS_CON14         0x024E
+#define MT6323_VSYS_CON15         0x0250
+#define MT6323_VSYS_CON18         0x0256
+#define MT6323_VPA_CON0           0x0300
+#define MT6323_VPA_CON1           0x0302
+#define MT6323_VPA_CON2           0x0304
+#define MT6323_VPA_CON3           0x0306
+#define MT6323_VPA_CON4           0x0308
+#define MT6323_VPA_CON5           0x030A
+#define MT6323_VPA_CON7           0x030E
+#define MT6323_VPA_CON8           0x0310
+#define MT6323_VPA_CON9           0x0312
+#define MT6323_VPA_CON10          0x0314
+#define MT6323_VPA_CON11          0x0316
+#define MT6323_VPA_CON12          0x0318
+#define MT6323_VPA_CON14          0x031C
+#define MT6323_VPA_CON16          0x0320
+#define MT6323_VPA_CON17          0x0322
+#define MT6323_VPA_CON18          0x0324
+#define MT6323_VPA_CON19          0x0326
+#define MT6323_VPA_CON20          0x0328
+#define MT6323_BUCK_K_CON0        0x032A
+#define MT6323_BUCK_K_CON1        0x032C
+#define MT6323_BUCK_K_CON2        0x032E
+#define MT6323_ISINK0_CON0        0x0330
+#define MT6323_ISINK0_CON1        0x0332
+#define MT6323_ISINK0_CON2        0x0334
+#define MT6323_ISINK0_CON3        0x0336
+#define MT6323_ISINK1_CON0        0x0338
+#define MT6323_ISINK1_CON1        0x033A
+#define MT6323_ISINK1_CON2        0x033C
+#define MT6323_ISINK1_CON3        0x033E
+#define MT6323_ISINK2_CON0        0x0340
+#define MT6323_ISINK2_CON1        0x0342
+#define MT6323_ISINK2_CON2        0x0344
+#define MT6323_ISINK2_CON3        0x0346
+#define MT6323_ISINK3_CON0        0x0348
+#define MT6323_ISINK3_CON1        0x034A
+#define MT6323_ISINK3_CON2        0x034C
+#define MT6323_ISINK3_CON3        0x034E
+#define MT6323_ISINK_ANA0         0x0350
+#define MT6323_ISINK_ANA1         0x0352
+#define MT6323_ISINK_PHASE_DLY    0x0354
+#define MT6323_ISINK_EN_CTRL      0x0356
+#define MT6323_ANALDO_CON0        0x0400
+#define MT6323_ANALDO_CON1        0x0402
+#define MT6323_ANALDO_CON2        0x0404
+#define MT6323_ANALDO_CON3        0x0406
+#define MT6323_ANALDO_CON4        0x0408
+#define MT6323_ANALDO_CON5        0x040A
+#define MT6323_ANALDO_CON6        0x040C
+#define MT6323_ANALDO_CON7        0x040E
+#define MT6323_ANALDO_CON8        0x0410
+#define MT6323_ANALDO_CON10       0x0412
+#define MT6323_ANALDO_CON15       0x0414
+#define MT6323_ANALDO_CON16       0x0416
+#define MT6323_ANALDO_CON17       0x0418
+#define MT6323_ANALDO_CON18       0x041A
+#define MT6323_ANALDO_CON19       0x041C
+#define MT6323_ANALDO_CON20       0x041E
+#define MT6323_ANALDO_CON21       0x0420
+#define MT6323_DIGLDO_CON0        0x0500
+#define MT6323_DIGLDO_CON2        0x0502
+#define MT6323_DIGLDO_CON3        0x0504
+#define MT6323_DIGLDO_CON5        0x0506
+#define MT6323_DIGLDO_CON6        0x0508
+#define MT6323_DIGLDO_CON7        0x050A
+#define MT6323_DIGLDO_CON8        0x050C
+#define MT6323_DIGLDO_CON9        0x050E
+#define MT6323_DIGLDO_CON10       0x0510
+#define MT6323_DIGLDO_CON11       0x0512
+#define MT6323_DIGLDO_CON12       0x0514
+#define MT6323_DIGLDO_CON13       0x0516
+#define MT6323_DIGLDO_CON14       0x0518
+#define MT6323_DIGLDO_CON15       0x051A
+#define MT6323_DIGLDO_CON16       0x051C
+#define MT6323_DIGLDO_CON17       0x051E
+#define MT6323_DIGLDO_CON18       0x0520
+#define MT6323_DIGLDO_CON19       0x0522
+#define MT6323_DIGLDO_CON20       0x0524
+#define MT6323_DIGLDO_CON21       0x0526
+#define MT6323_DIGLDO_CON23       0x0528
+#define MT6323_DIGLDO_CON24       0x052A
+#define MT6323_DIGLDO_CON26       0x052C
+#define MT6323_DIGLDO_CON27       0x052E
+#define MT6323_DIGLDO_CON28       0x0530
+#define MT6323_DIGLDO_CON29       0x0532
+#define MT6323_DIGLDO_CON30       0x0534
+#define MT6323_DIGLDO_CON31       0x0536
+#define MT6323_DIGLDO_CON32       0x0538
+#define MT6323_DIGLDO_CON33       0x053A
+#define MT6323_DIGLDO_CON34       0x053C
+#define MT6323_DIGLDO_CON35       0x053E
+#define MT6323_DIGLDO_CON36       0x0540
+#define MT6323_DIGLDO_CON39       0x0542
+#define MT6323_DIGLDO_CON40       0x0544
+#define MT6323_DIGLDO_CON41       0x0546
+#define MT6323_DIGLDO_CON42       0x0548
+#define MT6323_DIGLDO_CON43       0x054A
+#define MT6323_DIGLDO_CON44       0x054C
+#define MT6323_DIGLDO_CON45       0x054E
+#define MT6323_DIGLDO_CON46       0x0550
+#define MT6323_DIGLDO_CON47       0x0552
+#define MT6323_DIGLDO_CON48       0x0554
+#define MT6323_DIGLDO_CON49       0x0556
+#define MT6323_DIGLDO_CON50       0x0558
+#define MT6323_DIGLDO_CON51       0x055A
+#define MT6323_DIGLDO_CON52       0x055C
+#define MT6323_DIGLDO_CON53       0x055E
+#define MT6323_DIGLDO_CON54       0x0560
+#define MT6323_EFUSE_CON0         0x0600
+#define MT6323_EFUSE_CON1         0x0602
+#define MT6323_EFUSE_CON2         0x0604
+#define MT6323_EFUSE_CON3         0x0606
+#define MT6323_EFUSE_CON4         0x0608
+#define MT6323_EFUSE_CON5         0x060A
+#define MT6323_EFUSE_CON6         0x060C
+#define MT6323_EFUSE_VAL_0_15     0x060E
+#define MT6323_EFUSE_VAL_16_31    0x0610
+#define MT6323_EFUSE_VAL_32_47    0x0612
+#define MT6323_EFUSE_VAL_48_63    0x0614
+#define MT6323_EFUSE_VAL_64_79    0x0616
+#define MT6323_EFUSE_VAL_80_95    0x0618
+#define MT6323_EFUSE_VAL_96_111   0x061A
+#define MT6323_EFUSE_VAL_112_127  0x061C
+#define MT6323_EFUSE_VAL_128_143  0x061E
+#define MT6323_EFUSE_VAL_144_159  0x0620
+#define MT6323_EFUSE_VAL_160_175  0x0622
+#define MT6323_EFUSE_VAL_176_191  0x0624
+#define MT6323_EFUSE_DOUT_0_15    0x0626
+#define MT6323_EFUSE_DOUT_16_31   0x0628
+#define MT6323_EFUSE_DOUT_32_47   0x062A
+#define MT6323_EFUSE_DOUT_48_63   0x062C
+#define MT6323_EFUSE_DOUT_64_79   0x062E
+#define MT6323_EFUSE_DOUT_80_95   0x0630
+#define MT6323_EFUSE_DOUT_96_111  0x0632
+#define MT6323_EFUSE_DOUT_112_127 0x0634
+#define MT6323_EFUSE_DOUT_128_143 0x0636
+#define MT6323_EFUSE_DOUT_144_159 0x0638
+#define MT6323_EFUSE_DOUT_160_175 0x063A
+#define MT6323_EFUSE_DOUT_176_191 0x063C
+#define MT6323_EFUSE_CON7         0x063E
+#define MT6323_EFUSE_CON8         0x0640
+#define MT6323_EFUSE_CON9         0x0642
+#define MT6323_RTC_MIX_CON0       0x0644
+#define MT6323_RTC_MIX_CON1       0x0646
+#define MT6323_AUDTOP_CON0        0x0700
+#define MT6323_AUDTOP_CON1        0x0702
+#define MT6323_AUDTOP_CON2        0x0704
+#define MT6323_AUDTOP_CON3        0x0706
+#define MT6323_AUDTOP_CON4        0x0708
+#define MT6323_AUDTOP_CON5        0x070A
+#define MT6323_AUDTOP_CON6        0x070C
+#define MT6323_AUDTOP_CON7        0x070E
+#define MT6323_AUDTOP_CON8        0x0710
+#define MT6323_AUDTOP_CON9        0x0712
+#define MT6323_AUXADC_ADC0        0x0714
+#define MT6323_AUXADC_ADC1        0x0716
+#define MT6323_AUXADC_ADC2        0x0718
+#define MT6323_AUXADC_ADC3        0x071A
+#define MT6323_AUXADC_ADC4        0x071C
+#define MT6323_AUXADC_ADC5        0x071E
+#define MT6323_AUXADC_ADC6        0x0720
+#define MT6323_AUXADC_ADC7        0x0722
+#define MT6323_AUXADC_ADC8        0x0724
+#define MT6323_AUXADC_ADC9        0x0726
+#define MT6323_AUXADC_ADC10       0x0728
+#define MT6323_AUXADC_ADC11       0x072A
+#define MT6323_AUXADC_ADC12       0x072C
+#define MT6323_AUXADC_ADC13       0x072E
+#define MT6323_AUXADC_ADC14       0x0730
+#define MT6323_AUXADC_ADC15       0x0732
+#define MT6323_AUXADC_ADC16       0x0734
+#define MT6323_AUXADC_ADC17       0x0736
+#define MT6323_AUXADC_ADC18       0x0738
+#define MT6323_AUXADC_ADC19       0x073A
+#define MT6323_AUXADC_ADC20       0x073C
+#define MT6323_AUXADC_RSV1        0x073E
+#define MT6323_AUXADC_RSV2        0x0740
+#define MT6323_AUXADC_CON0        0x0742
+#define MT6323_AUXADC_CON1        0x0744
+#define MT6323_AUXADC_CON2        0x0746
+#define MT6323_AUXADC_CON3        0x0748
+#define MT6323_AUXADC_CON4        0x074A
+#define MT6323_AUXADC_CON5        0x074C
+#define MT6323_AUXADC_CON6        0x074E
+#define MT6323_AUXADC_CON7        0x0750
+#define MT6323_AUXADC_CON8        0x0752
+#define MT6323_AUXADC_CON9        0x0754
+#define MT6323_AUXADC_CON10       0x0756
+#define MT6323_AUXADC_CON11       0x0758
+#define MT6323_AUXADC_CON12       0x075A
+#define MT6323_AUXADC_CON13       0x075C
+#define MT6323_AUXADC_CON14       0x075E
+#define MT6323_AUXADC_CON15       0x0760
+#define MT6323_AUXADC_CON16       0x0762
+#define MT6323_AUXADC_CON17       0x0764
+#define MT6323_AUXADC_CON18       0x0766
+#define MT6323_AUXADC_CON19       0x0768
+#define MT6323_AUXADC_CON20       0x076A
+#define MT6323_AUXADC_CON21       0x076C
+#define MT6323_AUXADC_CON22       0x076E
+#define MT6323_AUXADC_CON23       0x0770
+#define MT6323_AUXADC_CON24       0x0772
+#define MT6323_AUXADC_CON25       0x0774
+#define MT6323_AUXADC_CON26       0x0776
+#define MT6323_AUXADC_CON27       0x0778
+#define MT6323_ACCDET_CON0        0x077A
+#define MT6323_ACCDET_CON1        0x077C
+#define MT6323_ACCDET_CON2        0x077E
+#define MT6323_ACCDET_CON3        0x0780
+#define MT6323_ACCDET_CON4        0x0782
+#define MT6323_ACCDET_CON5        0x0784
+#define MT6323_ACCDET_CON6        0x0786
+#define MT6323_ACCDET_CON7        0x0788
+#define MT6323_ACCDET_CON8        0x078A
+#define MT6323_ACCDET_CON9        0x078C
+#define MT6323_ACCDET_CON10       0x078E
+#define MT6323_ACCDET_CON11       0x0790
+#define MT6323_ACCDET_CON12       0x0792
+#define MT6323_ACCDET_CON13       0x0794
+#define MT6323_ACCDET_CON14       0x0796
+#define MT6323_ACCDET_CON15       0x0798
+#define MT6323_ACCDET_CON16       0x079A
+
+#endif /* __MFD_MT6323_REGISTERS_H__ */
-- 
1.7.10.4

