From 232754cb0ecd1967a8b72d6bd05467843d65a441 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Fri, 8 Jan 2016 13:42:06 +0000
Subject: [PATCH 127/170] FIXUP BCM270X_DT: "random" (HWRNG) dtparam default is
 on

---
 arch/arm/boot/dts/overlays/README | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/overlays/README
+++ b/arch/arm/boot/dts/overlays/README
@@ -110,7 +110,7 @@ Params:
                                  (default "off")
 
         random                   Set to "on" to enable the hardware random
-                                 number generator (default "off")
+                                 number generator (default "on")
 
         uart0                    Set to "off" to disable uart0 (default "on")
 
